#[doc = r" Register block"]
#[repr(C)]
pub struct RegisterBlock {
    #[doc = "0x00 - Control Register"]
    pub cr: CR,
    #[doc = "0x04 - Error Status Register"]
    pub es: ES,
    _reserved0: [u8; 4usize],
    #[doc = "0x0c - Enable Request Register"]
    pub erq: ERQ,
    _reserved1: [u8; 4usize],
    #[doc = "0x14 - Enable Error Interrupt Register"]
    pub eei: EEI,
    #[doc = "0x18 - Clear Enable Error Interrupt Register"]
    pub ceei: CEEI,
    #[doc = "0x19 - Set Enable Error Interrupt Register"]
    pub seei: SEEI,
    #[doc = "0x1a - Clear Enable Request Register"]
    pub cerq: CERQ,
    #[doc = "0x1b - Set Enable Request Register"]
    pub serq: SERQ,
    #[doc = "0x1c - Clear DONE Status Bit Register"]
    pub cdne: CDNE,
    #[doc = "0x1d - Set START Bit Register"]
    pub ssrt: SSRT,
    #[doc = "0x1e - Clear Error Register"]
    pub cerr: CERR,
    #[doc = "0x1f - Clear Interrupt Request Register"]
    pub cint: CINT,
    _reserved2: [u8; 4usize],
    #[doc = "0x24 - Interrupt Request Register"]
    pub int: INT,
    _reserved3: [u8; 4usize],
    #[doc = "0x2c - Error Register"]
    pub err: ERR,
    _reserved4: [u8; 4usize],
    #[doc = "0x34 - Hardware Request Status Register"]
    pub hrs: HRS,
    _reserved5: [u8; 12usize],
    #[doc = "0x44 - Enable Asynchronous Request in Stop Register"]
    pub ears: EARS,
    _reserved6: [u8; 184usize],
    #[doc = "0x100 - Channel n Priority Register"]
    pub dchpri3: DCHPRI3,
    #[doc = "0x101 - Channel n Priority Register"]
    pub dchpri2: DCHPRI2,
    #[doc = "0x102 - Channel n Priority Register"]
    pub dchpri1: DCHPRI1,
    #[doc = "0x103 - Channel n Priority Register"]
    pub dchpri0: DCHPRI0,
    #[doc = "0x104 - Channel n Priority Register"]
    pub dchpri7: DCHPRI7,
    #[doc = "0x105 - Channel n Priority Register"]
    pub dchpri6: DCHPRI6,
    #[doc = "0x106 - Channel n Priority Register"]
    pub dchpri5: DCHPRI5,
    #[doc = "0x107 - Channel n Priority Register"]
    pub dchpri4: DCHPRI4,
    #[doc = "0x108 - Channel n Priority Register"]
    pub dchpri11: DCHPRI11,
    #[doc = "0x109 - Channel n Priority Register"]
    pub dchpri10: DCHPRI10,
    #[doc = "0x10a - Channel n Priority Register"]
    pub dchpri9: DCHPRI9,
    #[doc = "0x10b - Channel n Priority Register"]
    pub dchpri8: DCHPRI8,
    #[doc = "0x10c - Channel n Priority Register"]
    pub dchpri15: DCHPRI15,
    #[doc = "0x10d - Channel n Priority Register"]
    pub dchpri14: DCHPRI14,
    #[doc = "0x10e - Channel n Priority Register"]
    pub dchpri13: DCHPRI13,
    #[doc = "0x10f - Channel n Priority Register"]
    pub dchpri12: DCHPRI12,
    #[doc = "0x110 - Channel n Priority Register"]
    pub dchpri19: DCHPRI19,
    #[doc = "0x111 - Channel n Priority Register"]
    pub dchpri18: DCHPRI18,
    #[doc = "0x112 - Channel n Priority Register"]
    pub dchpri17: DCHPRI17,
    #[doc = "0x113 - Channel n Priority Register"]
    pub dchpri16: DCHPRI16,
    #[doc = "0x114 - Channel n Priority Register"]
    pub dchpri23: DCHPRI23,
    #[doc = "0x115 - Channel n Priority Register"]
    pub dchpri22: DCHPRI22,
    #[doc = "0x116 - Channel n Priority Register"]
    pub dchpri21: DCHPRI21,
    #[doc = "0x117 - Channel n Priority Register"]
    pub dchpri20: DCHPRI20,
    #[doc = "0x118 - Channel n Priority Register"]
    pub dchpri27: DCHPRI27,
    #[doc = "0x119 - Channel n Priority Register"]
    pub dchpri26: DCHPRI26,
    #[doc = "0x11a - Channel n Priority Register"]
    pub dchpri25: DCHPRI25,
    #[doc = "0x11b - Channel n Priority Register"]
    pub dchpri24: DCHPRI24,
    #[doc = "0x11c - Channel n Priority Register"]
    pub dchpri31: DCHPRI31,
    #[doc = "0x11d - Channel n Priority Register"]
    pub dchpri30: DCHPRI30,
    #[doc = "0x11e - Channel n Priority Register"]
    pub dchpri29: DCHPRI29,
    #[doc = "0x11f - Channel n Priority Register"]
    pub dchpri28: DCHPRI28,
    _reserved7: [u8; 3808usize],
    #[doc = "0x1000 - TCD Source Address"]
    pub tcd0_saddr: TCD0_SADDR,
    #[doc = "0x1004 - TCD Signed Source Address Offset"]
    pub tcd0_soff: TCD0_SOFF,
    #[doc = "0x1006 - TCD Transfer Attributes"]
    pub tcd0_attr: TCD0_ATTR,
    #[doc = "0x1008 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd0_nbytes_mlno: TCD0_NBYTES_MLNO,
    #[doc = "0x100c - TCD Last Source Address Adjustment"]
    pub tcd0_slast: TCD0_SLAST,
    #[doc = "0x1010 - TCD Destination Address"]
    pub tcd0_daddr: TCD0_DADDR,
    #[doc = "0x1014 - TCD Signed Destination Address Offset"]
    pub tcd0_doff: TCD0_DOFF,
    #[doc = "0x1016 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd0_citer_elinkno: TCD0_CITER_ELINKNO,
    #[doc = "0x1018 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd0_dlastsga: TCD0_DLASTSGA,
    #[doc = "0x101c - TCD Control and Status"]
    pub tcd0_csr: TCD0_CSR,
    #[doc = "0x101e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd0_biter_elinkno: TCD0_BITER_ELINKNO,
    #[doc = "0x1020 - TCD Source Address"]
    pub tcd1_saddr: TCD1_SADDR,
    #[doc = "0x1024 - TCD Signed Source Address Offset"]
    pub tcd1_soff: TCD1_SOFF,
    #[doc = "0x1026 - TCD Transfer Attributes"]
    pub tcd1_attr: TCD1_ATTR,
    #[doc = "0x1028 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd1_nbytes_mlno: TCD1_NBYTES_MLNO,
    #[doc = "0x102c - TCD Last Source Address Adjustment"]
    pub tcd1_slast: TCD1_SLAST,
    #[doc = "0x1030 - TCD Destination Address"]
    pub tcd1_daddr: TCD1_DADDR,
    #[doc = "0x1034 - TCD Signed Destination Address Offset"]
    pub tcd1_doff: TCD1_DOFF,
    #[doc = "0x1036 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd1_citer_elinkno: TCD1_CITER_ELINKNO,
    #[doc = "0x1038 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd1_dlastsga: TCD1_DLASTSGA,
    #[doc = "0x103c - TCD Control and Status"]
    pub tcd1_csr: TCD1_CSR,
    #[doc = "0x103e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd1_biter_elinkno: TCD1_BITER_ELINKNO,
    #[doc = "0x1040 - TCD Source Address"]
    pub tcd2_saddr: TCD2_SADDR,
    #[doc = "0x1044 - TCD Signed Source Address Offset"]
    pub tcd2_soff: TCD2_SOFF,
    #[doc = "0x1046 - TCD Transfer Attributes"]
    pub tcd2_attr: TCD2_ATTR,
    #[doc = "0x1048 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd2_nbytes_mlno: TCD2_NBYTES_MLNO,
    #[doc = "0x104c - TCD Last Source Address Adjustment"]
    pub tcd2_slast: TCD2_SLAST,
    #[doc = "0x1050 - TCD Destination Address"]
    pub tcd2_daddr: TCD2_DADDR,
    #[doc = "0x1054 - TCD Signed Destination Address Offset"]
    pub tcd2_doff: TCD2_DOFF,
    #[doc = "0x1056 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd2_citer_elinkno: TCD2_CITER_ELINKNO,
    #[doc = "0x1058 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd2_dlastsga: TCD2_DLASTSGA,
    #[doc = "0x105c - TCD Control and Status"]
    pub tcd2_csr: TCD2_CSR,
    #[doc = "0x105e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd2_biter_elinkno: TCD2_BITER_ELINKNO,
    #[doc = "0x1060 - TCD Source Address"]
    pub tcd3_saddr: TCD3_SADDR,
    #[doc = "0x1064 - TCD Signed Source Address Offset"]
    pub tcd3_soff: TCD3_SOFF,
    #[doc = "0x1066 - TCD Transfer Attributes"]
    pub tcd3_attr: TCD3_ATTR,
    #[doc = "0x1068 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd3_nbytes_mlno: TCD3_NBYTES_MLNO,
    #[doc = "0x106c - TCD Last Source Address Adjustment"]
    pub tcd3_slast: TCD3_SLAST,
    #[doc = "0x1070 - TCD Destination Address"]
    pub tcd3_daddr: TCD3_DADDR,
    #[doc = "0x1074 - TCD Signed Destination Address Offset"]
    pub tcd3_doff: TCD3_DOFF,
    #[doc = "0x1076 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd3_citer_elinkno: TCD3_CITER_ELINKNO,
    #[doc = "0x1078 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd3_dlastsga: TCD3_DLASTSGA,
    #[doc = "0x107c - TCD Control and Status"]
    pub tcd3_csr: TCD3_CSR,
    #[doc = "0x107e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd3_biter_elinkno: TCD3_BITER_ELINKNO,
    #[doc = "0x1080 - TCD Source Address"]
    pub tcd4_saddr: TCD4_SADDR,
    #[doc = "0x1084 - TCD Signed Source Address Offset"]
    pub tcd4_soff: TCD4_SOFF,
    #[doc = "0x1086 - TCD Transfer Attributes"]
    pub tcd4_attr: TCD4_ATTR,
    #[doc = "0x1088 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd4_nbytes_mlno: TCD4_NBYTES_MLNO,
    #[doc = "0x108c - TCD Last Source Address Adjustment"]
    pub tcd4_slast: TCD4_SLAST,
    #[doc = "0x1090 - TCD Destination Address"]
    pub tcd4_daddr: TCD4_DADDR,
    #[doc = "0x1094 - TCD Signed Destination Address Offset"]
    pub tcd4_doff: TCD4_DOFF,
    #[doc = "0x1096 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd4_citer_elinkno: TCD4_CITER_ELINKNO,
    #[doc = "0x1098 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd4_dlastsga: TCD4_DLASTSGA,
    #[doc = "0x109c - TCD Control and Status"]
    pub tcd4_csr: TCD4_CSR,
    #[doc = "0x109e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd4_biter_elinkno: TCD4_BITER_ELINKNO,
    #[doc = "0x10a0 - TCD Source Address"]
    pub tcd5_saddr: TCD5_SADDR,
    #[doc = "0x10a4 - TCD Signed Source Address Offset"]
    pub tcd5_soff: TCD5_SOFF,
    #[doc = "0x10a6 - TCD Transfer Attributes"]
    pub tcd5_attr: TCD5_ATTR,
    #[doc = "0x10a8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd5_nbytes_mlno: TCD5_NBYTES_MLNO,
    #[doc = "0x10ac - TCD Last Source Address Adjustment"]
    pub tcd5_slast: TCD5_SLAST,
    #[doc = "0x10b0 - TCD Destination Address"]
    pub tcd5_daddr: TCD5_DADDR,
    #[doc = "0x10b4 - TCD Signed Destination Address Offset"]
    pub tcd5_doff: TCD5_DOFF,
    #[doc = "0x10b6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd5_citer_elinkno: TCD5_CITER_ELINKNO,
    #[doc = "0x10b8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd5_dlastsga: TCD5_DLASTSGA,
    #[doc = "0x10bc - TCD Control and Status"]
    pub tcd5_csr: TCD5_CSR,
    #[doc = "0x10be - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd5_biter_elinkno: TCD5_BITER_ELINKNO,
    #[doc = "0x10c0 - TCD Source Address"]
    pub tcd6_saddr: TCD6_SADDR,
    #[doc = "0x10c4 - TCD Signed Source Address Offset"]
    pub tcd6_soff: TCD6_SOFF,
    #[doc = "0x10c6 - TCD Transfer Attributes"]
    pub tcd6_attr: TCD6_ATTR,
    #[doc = "0x10c8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd6_nbytes_mlno: TCD6_NBYTES_MLNO,
    #[doc = "0x10cc - TCD Last Source Address Adjustment"]
    pub tcd6_slast: TCD6_SLAST,
    #[doc = "0x10d0 - TCD Destination Address"]
    pub tcd6_daddr: TCD6_DADDR,
    #[doc = "0x10d4 - TCD Signed Destination Address Offset"]
    pub tcd6_doff: TCD6_DOFF,
    #[doc = "0x10d6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd6_citer_elinkno: TCD6_CITER_ELINKNO,
    #[doc = "0x10d8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd6_dlastsga: TCD6_DLASTSGA,
    #[doc = "0x10dc - TCD Control and Status"]
    pub tcd6_csr: TCD6_CSR,
    #[doc = "0x10de - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd6_biter_elinkno: TCD6_BITER_ELINKNO,
    #[doc = "0x10e0 - TCD Source Address"]
    pub tcd7_saddr: TCD7_SADDR,
    #[doc = "0x10e4 - TCD Signed Source Address Offset"]
    pub tcd7_soff: TCD7_SOFF,
    #[doc = "0x10e6 - TCD Transfer Attributes"]
    pub tcd7_attr: TCD7_ATTR,
    #[doc = "0x10e8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd7_nbytes_mlno: TCD7_NBYTES_MLNO,
    #[doc = "0x10ec - TCD Last Source Address Adjustment"]
    pub tcd7_slast: TCD7_SLAST,
    #[doc = "0x10f0 - TCD Destination Address"]
    pub tcd7_daddr: TCD7_DADDR,
    #[doc = "0x10f4 - TCD Signed Destination Address Offset"]
    pub tcd7_doff: TCD7_DOFF,
    #[doc = "0x10f6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd7_citer_elinkno: TCD7_CITER_ELINKNO,
    #[doc = "0x10f8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd7_dlastsga: TCD7_DLASTSGA,
    #[doc = "0x10fc - TCD Control and Status"]
    pub tcd7_csr: TCD7_CSR,
    #[doc = "0x10fe - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd7_biter_elinkno: TCD7_BITER_ELINKNO,
    #[doc = "0x1100 - TCD Source Address"]
    pub tcd8_saddr: TCD8_SADDR,
    #[doc = "0x1104 - TCD Signed Source Address Offset"]
    pub tcd8_soff: TCD8_SOFF,
    #[doc = "0x1106 - TCD Transfer Attributes"]
    pub tcd8_attr: TCD8_ATTR,
    #[doc = "0x1108 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd8_nbytes_mlno: TCD8_NBYTES_MLNO,
    #[doc = "0x110c - TCD Last Source Address Adjustment"]
    pub tcd8_slast: TCD8_SLAST,
    #[doc = "0x1110 - TCD Destination Address"]
    pub tcd8_daddr: TCD8_DADDR,
    #[doc = "0x1114 - TCD Signed Destination Address Offset"]
    pub tcd8_doff: TCD8_DOFF,
    #[doc = "0x1116 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd8_citer_elinkno: TCD8_CITER_ELINKNO,
    #[doc = "0x1118 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd8_dlastsga: TCD8_DLASTSGA,
    #[doc = "0x111c - TCD Control and Status"]
    pub tcd8_csr: TCD8_CSR,
    #[doc = "0x111e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd8_biter_elinkno: TCD8_BITER_ELINKNO,
    #[doc = "0x1120 - TCD Source Address"]
    pub tcd9_saddr: TCD9_SADDR,
    #[doc = "0x1124 - TCD Signed Source Address Offset"]
    pub tcd9_soff: TCD9_SOFF,
    #[doc = "0x1126 - TCD Transfer Attributes"]
    pub tcd9_attr: TCD9_ATTR,
    #[doc = "0x1128 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd9_nbytes_mlno: TCD9_NBYTES_MLNO,
    #[doc = "0x112c - TCD Last Source Address Adjustment"]
    pub tcd9_slast: TCD9_SLAST,
    #[doc = "0x1130 - TCD Destination Address"]
    pub tcd9_daddr: TCD9_DADDR,
    #[doc = "0x1134 - TCD Signed Destination Address Offset"]
    pub tcd9_doff: TCD9_DOFF,
    #[doc = "0x1136 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd9_citer_elinkno: TCD9_CITER_ELINKNO,
    #[doc = "0x1138 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd9_dlastsga: TCD9_DLASTSGA,
    #[doc = "0x113c - TCD Control and Status"]
    pub tcd9_csr: TCD9_CSR,
    #[doc = "0x113e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd9_biter_elinkno: TCD9_BITER_ELINKNO,
    #[doc = "0x1140 - TCD Source Address"]
    pub tcd10_saddr: TCD10_SADDR,
    #[doc = "0x1144 - TCD Signed Source Address Offset"]
    pub tcd10_soff: TCD10_SOFF,
    #[doc = "0x1146 - TCD Transfer Attributes"]
    pub tcd10_attr: TCD10_ATTR,
    #[doc = "0x1148 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd10_nbytes_mlno: TCD10_NBYTES_MLNO,
    #[doc = "0x114c - TCD Last Source Address Adjustment"]
    pub tcd10_slast: TCD10_SLAST,
    #[doc = "0x1150 - TCD Destination Address"]
    pub tcd10_daddr: TCD10_DADDR,
    #[doc = "0x1154 - TCD Signed Destination Address Offset"]
    pub tcd10_doff: TCD10_DOFF,
    #[doc = "0x1156 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd10_citer_elinkno: TCD10_CITER_ELINKNO,
    #[doc = "0x1158 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd10_dlastsga: TCD10_DLASTSGA,
    #[doc = "0x115c - TCD Control and Status"]
    pub tcd10_csr: TCD10_CSR,
    #[doc = "0x115e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd10_biter_elinkno: TCD10_BITER_ELINKNO,
    #[doc = "0x1160 - TCD Source Address"]
    pub tcd11_saddr: TCD11_SADDR,
    #[doc = "0x1164 - TCD Signed Source Address Offset"]
    pub tcd11_soff: TCD11_SOFF,
    #[doc = "0x1166 - TCD Transfer Attributes"]
    pub tcd11_attr: TCD11_ATTR,
    #[doc = "0x1168 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd11_nbytes_mlno: TCD11_NBYTES_MLNO,
    #[doc = "0x116c - TCD Last Source Address Adjustment"]
    pub tcd11_slast: TCD11_SLAST,
    #[doc = "0x1170 - TCD Destination Address"]
    pub tcd11_daddr: TCD11_DADDR,
    #[doc = "0x1174 - TCD Signed Destination Address Offset"]
    pub tcd11_doff: TCD11_DOFF,
    #[doc = "0x1176 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd11_citer_elinkno: TCD11_CITER_ELINKNO,
    #[doc = "0x1178 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd11_dlastsga: TCD11_DLASTSGA,
    #[doc = "0x117c - TCD Control and Status"]
    pub tcd11_csr: TCD11_CSR,
    #[doc = "0x117e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd11_biter_elinkno: TCD11_BITER_ELINKNO,
    #[doc = "0x1180 - TCD Source Address"]
    pub tcd12_saddr: TCD12_SADDR,
    #[doc = "0x1184 - TCD Signed Source Address Offset"]
    pub tcd12_soff: TCD12_SOFF,
    #[doc = "0x1186 - TCD Transfer Attributes"]
    pub tcd12_attr: TCD12_ATTR,
    #[doc = "0x1188 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd12_nbytes_mlno: TCD12_NBYTES_MLNO,
    #[doc = "0x118c - TCD Last Source Address Adjustment"]
    pub tcd12_slast: TCD12_SLAST,
    #[doc = "0x1190 - TCD Destination Address"]
    pub tcd12_daddr: TCD12_DADDR,
    #[doc = "0x1194 - TCD Signed Destination Address Offset"]
    pub tcd12_doff: TCD12_DOFF,
    #[doc = "0x1196 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd12_citer_elinkno: TCD12_CITER_ELINKNO,
    #[doc = "0x1198 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd12_dlastsga: TCD12_DLASTSGA,
    #[doc = "0x119c - TCD Control and Status"]
    pub tcd12_csr: TCD12_CSR,
    #[doc = "0x119e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd12_biter_elinkno: TCD12_BITER_ELINKNO,
    #[doc = "0x11a0 - TCD Source Address"]
    pub tcd13_saddr: TCD13_SADDR,
    #[doc = "0x11a4 - TCD Signed Source Address Offset"]
    pub tcd13_soff: TCD13_SOFF,
    #[doc = "0x11a6 - TCD Transfer Attributes"]
    pub tcd13_attr: TCD13_ATTR,
    #[doc = "0x11a8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd13_nbytes_mlno: TCD13_NBYTES_MLNO,
    #[doc = "0x11ac - TCD Last Source Address Adjustment"]
    pub tcd13_slast: TCD13_SLAST,
    #[doc = "0x11b0 - TCD Destination Address"]
    pub tcd13_daddr: TCD13_DADDR,
    #[doc = "0x11b4 - TCD Signed Destination Address Offset"]
    pub tcd13_doff: TCD13_DOFF,
    #[doc = "0x11b6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd13_citer_elinkno: TCD13_CITER_ELINKNO,
    #[doc = "0x11b8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd13_dlastsga: TCD13_DLASTSGA,
    #[doc = "0x11bc - TCD Control and Status"]
    pub tcd13_csr: TCD13_CSR,
    #[doc = "0x11be - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd13_biter_elinkno: TCD13_BITER_ELINKNO,
    #[doc = "0x11c0 - TCD Source Address"]
    pub tcd14_saddr: TCD14_SADDR,
    #[doc = "0x11c4 - TCD Signed Source Address Offset"]
    pub tcd14_soff: TCD14_SOFF,
    #[doc = "0x11c6 - TCD Transfer Attributes"]
    pub tcd14_attr: TCD14_ATTR,
    #[doc = "0x11c8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd14_nbytes_mlno: TCD14_NBYTES_MLNO,
    #[doc = "0x11cc - TCD Last Source Address Adjustment"]
    pub tcd14_slast: TCD14_SLAST,
    #[doc = "0x11d0 - TCD Destination Address"]
    pub tcd14_daddr: TCD14_DADDR,
    #[doc = "0x11d4 - TCD Signed Destination Address Offset"]
    pub tcd14_doff: TCD14_DOFF,
    #[doc = "0x11d6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd14_citer_elinkno: TCD14_CITER_ELINKNO,
    #[doc = "0x11d8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd14_dlastsga: TCD14_DLASTSGA,
    #[doc = "0x11dc - TCD Control and Status"]
    pub tcd14_csr: TCD14_CSR,
    #[doc = "0x11de - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd14_biter_elinkno: TCD14_BITER_ELINKNO,
    #[doc = "0x11e0 - TCD Source Address"]
    pub tcd15_saddr: TCD15_SADDR,
    #[doc = "0x11e4 - TCD Signed Source Address Offset"]
    pub tcd15_soff: TCD15_SOFF,
    #[doc = "0x11e6 - TCD Transfer Attributes"]
    pub tcd15_attr: TCD15_ATTR,
    #[doc = "0x11e8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd15_nbytes_mlno: TCD15_NBYTES_MLNO,
    #[doc = "0x11ec - TCD Last Source Address Adjustment"]
    pub tcd15_slast: TCD15_SLAST,
    #[doc = "0x11f0 - TCD Destination Address"]
    pub tcd15_daddr: TCD15_DADDR,
    #[doc = "0x11f4 - TCD Signed Destination Address Offset"]
    pub tcd15_doff: TCD15_DOFF,
    #[doc = "0x11f6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd15_citer_elinkno: TCD15_CITER_ELINKNO,
    #[doc = "0x11f8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd15_dlastsga: TCD15_DLASTSGA,
    #[doc = "0x11fc - TCD Control and Status"]
    pub tcd15_csr: TCD15_CSR,
    #[doc = "0x11fe - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd15_biter_elinkno: TCD15_BITER_ELINKNO,
    #[doc = "0x1200 - TCD Source Address"]
    pub tcd16_saddr: TCD16_SADDR,
    #[doc = "0x1204 - TCD Signed Source Address Offset"]
    pub tcd16_soff: TCD16_SOFF,
    #[doc = "0x1206 - TCD Transfer Attributes"]
    pub tcd16_attr: TCD16_ATTR,
    #[doc = "0x1208 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd16_nbytes_mlno: TCD16_NBYTES_MLNO,
    #[doc = "0x120c - TCD Last Source Address Adjustment"]
    pub tcd16_slast: TCD16_SLAST,
    #[doc = "0x1210 - TCD Destination Address"]
    pub tcd16_daddr: TCD16_DADDR,
    #[doc = "0x1214 - TCD Signed Destination Address Offset"]
    pub tcd16_doff: TCD16_DOFF,
    #[doc = "0x1216 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd16_citer_elinkno: TCD16_CITER_ELINKNO,
    #[doc = "0x1218 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd16_dlastsga: TCD16_DLASTSGA,
    #[doc = "0x121c - TCD Control and Status"]
    pub tcd16_csr: TCD16_CSR,
    #[doc = "0x121e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd16_biter_elinkno: TCD16_BITER_ELINKNO,
    #[doc = "0x1220 - TCD Source Address"]
    pub tcd17_saddr: TCD17_SADDR,
    #[doc = "0x1224 - TCD Signed Source Address Offset"]
    pub tcd17_soff: TCD17_SOFF,
    #[doc = "0x1226 - TCD Transfer Attributes"]
    pub tcd17_attr: TCD17_ATTR,
    #[doc = "0x1228 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd17_nbytes_mlno: TCD17_NBYTES_MLNO,
    #[doc = "0x122c - TCD Last Source Address Adjustment"]
    pub tcd17_slast: TCD17_SLAST,
    #[doc = "0x1230 - TCD Destination Address"]
    pub tcd17_daddr: TCD17_DADDR,
    #[doc = "0x1234 - TCD Signed Destination Address Offset"]
    pub tcd17_doff: TCD17_DOFF,
    #[doc = "0x1236 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd17_citer_elinkno: TCD17_CITER_ELINKNO,
    #[doc = "0x1238 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd17_dlastsga: TCD17_DLASTSGA,
    #[doc = "0x123c - TCD Control and Status"]
    pub tcd17_csr: TCD17_CSR,
    #[doc = "0x123e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd17_biter_elinkno: TCD17_BITER_ELINKNO,
    #[doc = "0x1240 - TCD Source Address"]
    pub tcd18_saddr: TCD18_SADDR,
    #[doc = "0x1244 - TCD Signed Source Address Offset"]
    pub tcd18_soff: TCD18_SOFF,
    #[doc = "0x1246 - TCD Transfer Attributes"]
    pub tcd18_attr: TCD18_ATTR,
    #[doc = "0x1248 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd18_nbytes_mlno: TCD18_NBYTES_MLNO,
    #[doc = "0x124c - TCD Last Source Address Adjustment"]
    pub tcd18_slast: TCD18_SLAST,
    #[doc = "0x1250 - TCD Destination Address"]
    pub tcd18_daddr: TCD18_DADDR,
    #[doc = "0x1254 - TCD Signed Destination Address Offset"]
    pub tcd18_doff: TCD18_DOFF,
    #[doc = "0x1256 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd18_citer_elinkno: TCD18_CITER_ELINKNO,
    #[doc = "0x1258 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd18_dlastsga: TCD18_DLASTSGA,
    #[doc = "0x125c - TCD Control and Status"]
    pub tcd18_csr: TCD18_CSR,
    #[doc = "0x125e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd18_biter_elinkno: TCD18_BITER_ELINKNO,
    #[doc = "0x1260 - TCD Source Address"]
    pub tcd19_saddr: TCD19_SADDR,
    #[doc = "0x1264 - TCD Signed Source Address Offset"]
    pub tcd19_soff: TCD19_SOFF,
    #[doc = "0x1266 - TCD Transfer Attributes"]
    pub tcd19_attr: TCD19_ATTR,
    #[doc = "0x1268 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd19_nbytes_mlno: TCD19_NBYTES_MLNO,
    #[doc = "0x126c - TCD Last Source Address Adjustment"]
    pub tcd19_slast: TCD19_SLAST,
    #[doc = "0x1270 - TCD Destination Address"]
    pub tcd19_daddr: TCD19_DADDR,
    #[doc = "0x1274 - TCD Signed Destination Address Offset"]
    pub tcd19_doff: TCD19_DOFF,
    #[doc = "0x1276 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd19_citer_elinkno: TCD19_CITER_ELINKNO,
    #[doc = "0x1278 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd19_dlastsga: TCD19_DLASTSGA,
    #[doc = "0x127c - TCD Control and Status"]
    pub tcd19_csr: TCD19_CSR,
    #[doc = "0x127e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd19_biter_elinkno: TCD19_BITER_ELINKNO,
    #[doc = "0x1280 - TCD Source Address"]
    pub tcd20_saddr: TCD20_SADDR,
    #[doc = "0x1284 - TCD Signed Source Address Offset"]
    pub tcd20_soff: TCD20_SOFF,
    #[doc = "0x1286 - TCD Transfer Attributes"]
    pub tcd20_attr: TCD20_ATTR,
    #[doc = "0x1288 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd20_nbytes_mlno: TCD20_NBYTES_MLNO,
    #[doc = "0x128c - TCD Last Source Address Adjustment"]
    pub tcd20_slast: TCD20_SLAST,
    #[doc = "0x1290 - TCD Destination Address"]
    pub tcd20_daddr: TCD20_DADDR,
    #[doc = "0x1294 - TCD Signed Destination Address Offset"]
    pub tcd20_doff: TCD20_DOFF,
    #[doc = "0x1296 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd20_citer_elinkno: TCD20_CITER_ELINKNO,
    #[doc = "0x1298 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd20_dlastsga: TCD20_DLASTSGA,
    #[doc = "0x129c - TCD Control and Status"]
    pub tcd20_csr: TCD20_CSR,
    #[doc = "0x129e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd20_biter_elinkno: TCD20_BITER_ELINKNO,
    #[doc = "0x12a0 - TCD Source Address"]
    pub tcd21_saddr: TCD21_SADDR,
    #[doc = "0x12a4 - TCD Signed Source Address Offset"]
    pub tcd21_soff: TCD21_SOFF,
    #[doc = "0x12a6 - TCD Transfer Attributes"]
    pub tcd21_attr: TCD21_ATTR,
    #[doc = "0x12a8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd21_nbytes_mlno: TCD21_NBYTES_MLNO,
    #[doc = "0x12ac - TCD Last Source Address Adjustment"]
    pub tcd21_slast: TCD21_SLAST,
    #[doc = "0x12b0 - TCD Destination Address"]
    pub tcd21_daddr: TCD21_DADDR,
    #[doc = "0x12b4 - TCD Signed Destination Address Offset"]
    pub tcd21_doff: TCD21_DOFF,
    #[doc = "0x12b6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd21_citer_elinkno: TCD21_CITER_ELINKNO,
    #[doc = "0x12b8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd21_dlastsga: TCD21_DLASTSGA,
    #[doc = "0x12bc - TCD Control and Status"]
    pub tcd21_csr: TCD21_CSR,
    #[doc = "0x12be - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd21_biter_elinkno: TCD21_BITER_ELINKNO,
    #[doc = "0x12c0 - TCD Source Address"]
    pub tcd22_saddr: TCD22_SADDR,
    #[doc = "0x12c4 - TCD Signed Source Address Offset"]
    pub tcd22_soff: TCD22_SOFF,
    #[doc = "0x12c6 - TCD Transfer Attributes"]
    pub tcd22_attr: TCD22_ATTR,
    #[doc = "0x12c8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd22_nbytes_mlno: TCD22_NBYTES_MLNO,
    #[doc = "0x12cc - TCD Last Source Address Adjustment"]
    pub tcd22_slast: TCD22_SLAST,
    #[doc = "0x12d0 - TCD Destination Address"]
    pub tcd22_daddr: TCD22_DADDR,
    #[doc = "0x12d4 - TCD Signed Destination Address Offset"]
    pub tcd22_doff: TCD22_DOFF,
    #[doc = "0x12d6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd22_citer_elinkno: TCD22_CITER_ELINKNO,
    #[doc = "0x12d8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd22_dlastsga: TCD22_DLASTSGA,
    #[doc = "0x12dc - TCD Control and Status"]
    pub tcd22_csr: TCD22_CSR,
    #[doc = "0x12de - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd22_biter_elinkno: TCD22_BITER_ELINKNO,
    #[doc = "0x12e0 - TCD Source Address"]
    pub tcd23_saddr: TCD23_SADDR,
    #[doc = "0x12e4 - TCD Signed Source Address Offset"]
    pub tcd23_soff: TCD23_SOFF,
    #[doc = "0x12e6 - TCD Transfer Attributes"]
    pub tcd23_attr: TCD23_ATTR,
    #[doc = "0x12e8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd23_nbytes_mlno: TCD23_NBYTES_MLNO,
    #[doc = "0x12ec - TCD Last Source Address Adjustment"]
    pub tcd23_slast: TCD23_SLAST,
    #[doc = "0x12f0 - TCD Destination Address"]
    pub tcd23_daddr: TCD23_DADDR,
    #[doc = "0x12f4 - TCD Signed Destination Address Offset"]
    pub tcd23_doff: TCD23_DOFF,
    #[doc = "0x12f6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd23_citer_elinkno: TCD23_CITER_ELINKNO,
    #[doc = "0x12f8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd23_dlastsga: TCD23_DLASTSGA,
    #[doc = "0x12fc - TCD Control and Status"]
    pub tcd23_csr: TCD23_CSR,
    #[doc = "0x12fe - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd23_biter_elinkno: TCD23_BITER_ELINKNO,
    #[doc = "0x1300 - TCD Source Address"]
    pub tcd24_saddr: TCD24_SADDR,
    #[doc = "0x1304 - TCD Signed Source Address Offset"]
    pub tcd24_soff: TCD24_SOFF,
    #[doc = "0x1306 - TCD Transfer Attributes"]
    pub tcd24_attr: TCD24_ATTR,
    #[doc = "0x1308 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd24_nbytes_mlno: TCD24_NBYTES_MLNO,
    #[doc = "0x130c - TCD Last Source Address Adjustment"]
    pub tcd24_slast: TCD24_SLAST,
    #[doc = "0x1310 - TCD Destination Address"]
    pub tcd24_daddr: TCD24_DADDR,
    #[doc = "0x1314 - TCD Signed Destination Address Offset"]
    pub tcd24_doff: TCD24_DOFF,
    #[doc = "0x1316 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd24_citer_elinkno: TCD24_CITER_ELINKNO,
    #[doc = "0x1318 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd24_dlastsga: TCD24_DLASTSGA,
    #[doc = "0x131c - TCD Control and Status"]
    pub tcd24_csr: TCD24_CSR,
    #[doc = "0x131e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd24_biter_elinkno: TCD24_BITER_ELINKNO,
    #[doc = "0x1320 - TCD Source Address"]
    pub tcd25_saddr: TCD25_SADDR,
    #[doc = "0x1324 - TCD Signed Source Address Offset"]
    pub tcd25_soff: TCD25_SOFF,
    #[doc = "0x1326 - TCD Transfer Attributes"]
    pub tcd25_attr: TCD25_ATTR,
    #[doc = "0x1328 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd25_nbytes_mlno: TCD25_NBYTES_MLNO,
    #[doc = "0x132c - TCD Last Source Address Adjustment"]
    pub tcd25_slast: TCD25_SLAST,
    #[doc = "0x1330 - TCD Destination Address"]
    pub tcd25_daddr: TCD25_DADDR,
    #[doc = "0x1334 - TCD Signed Destination Address Offset"]
    pub tcd25_doff: TCD25_DOFF,
    #[doc = "0x1336 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd25_citer_elinkno: TCD25_CITER_ELINKNO,
    #[doc = "0x1338 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd25_dlastsga: TCD25_DLASTSGA,
    #[doc = "0x133c - TCD Control and Status"]
    pub tcd25_csr: TCD25_CSR,
    #[doc = "0x133e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd25_biter_elinkno: TCD25_BITER_ELINKNO,
    #[doc = "0x1340 - TCD Source Address"]
    pub tcd26_saddr: TCD26_SADDR,
    #[doc = "0x1344 - TCD Signed Source Address Offset"]
    pub tcd26_soff: TCD26_SOFF,
    #[doc = "0x1346 - TCD Transfer Attributes"]
    pub tcd26_attr: TCD26_ATTR,
    #[doc = "0x1348 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd26_nbytes_mlno: TCD26_NBYTES_MLNO,
    #[doc = "0x134c - TCD Last Source Address Adjustment"]
    pub tcd26_slast: TCD26_SLAST,
    #[doc = "0x1350 - TCD Destination Address"]
    pub tcd26_daddr: TCD26_DADDR,
    #[doc = "0x1354 - TCD Signed Destination Address Offset"]
    pub tcd26_doff: TCD26_DOFF,
    #[doc = "0x1356 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd26_citer_elinkno: TCD26_CITER_ELINKNO,
    #[doc = "0x1358 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd26_dlastsga: TCD26_DLASTSGA,
    #[doc = "0x135c - TCD Control and Status"]
    pub tcd26_csr: TCD26_CSR,
    #[doc = "0x135e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd26_biter_elinkno: TCD26_BITER_ELINKNO,
    #[doc = "0x1360 - TCD Source Address"]
    pub tcd27_saddr: TCD27_SADDR,
    #[doc = "0x1364 - TCD Signed Source Address Offset"]
    pub tcd27_soff: TCD27_SOFF,
    #[doc = "0x1366 - TCD Transfer Attributes"]
    pub tcd27_attr: TCD27_ATTR,
    #[doc = "0x1368 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd27_nbytes_mlno: TCD27_NBYTES_MLNO,
    #[doc = "0x136c - TCD Last Source Address Adjustment"]
    pub tcd27_slast: TCD27_SLAST,
    #[doc = "0x1370 - TCD Destination Address"]
    pub tcd27_daddr: TCD27_DADDR,
    #[doc = "0x1374 - TCD Signed Destination Address Offset"]
    pub tcd27_doff: TCD27_DOFF,
    #[doc = "0x1376 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd27_citer_elinkno: TCD27_CITER_ELINKNO,
    #[doc = "0x1378 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd27_dlastsga: TCD27_DLASTSGA,
    #[doc = "0x137c - TCD Control and Status"]
    pub tcd27_csr: TCD27_CSR,
    #[doc = "0x137e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd27_biter_elinkno: TCD27_BITER_ELINKNO,
    #[doc = "0x1380 - TCD Source Address"]
    pub tcd28_saddr: TCD28_SADDR,
    #[doc = "0x1384 - TCD Signed Source Address Offset"]
    pub tcd28_soff: TCD28_SOFF,
    #[doc = "0x1386 - TCD Transfer Attributes"]
    pub tcd28_attr: TCD28_ATTR,
    #[doc = "0x1388 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd28_nbytes_mlno: TCD28_NBYTES_MLNO,
    #[doc = "0x138c - TCD Last Source Address Adjustment"]
    pub tcd28_slast: TCD28_SLAST,
    #[doc = "0x1390 - TCD Destination Address"]
    pub tcd28_daddr: TCD28_DADDR,
    #[doc = "0x1394 - TCD Signed Destination Address Offset"]
    pub tcd28_doff: TCD28_DOFF,
    #[doc = "0x1396 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd28_citer_elinkno: TCD28_CITER_ELINKNO,
    #[doc = "0x1398 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd28_dlastsga: TCD28_DLASTSGA,
    #[doc = "0x139c - TCD Control and Status"]
    pub tcd28_csr: TCD28_CSR,
    #[doc = "0x139e - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd28_biter_elinkno: TCD28_BITER_ELINKNO,
    #[doc = "0x13a0 - TCD Source Address"]
    pub tcd29_saddr: TCD29_SADDR,
    #[doc = "0x13a4 - TCD Signed Source Address Offset"]
    pub tcd29_soff: TCD29_SOFF,
    #[doc = "0x13a6 - TCD Transfer Attributes"]
    pub tcd29_attr: TCD29_ATTR,
    #[doc = "0x13a8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd29_nbytes_mlno: TCD29_NBYTES_MLNO,
    #[doc = "0x13ac - TCD Last Source Address Adjustment"]
    pub tcd29_slast: TCD29_SLAST,
    #[doc = "0x13b0 - TCD Destination Address"]
    pub tcd29_daddr: TCD29_DADDR,
    #[doc = "0x13b4 - TCD Signed Destination Address Offset"]
    pub tcd29_doff: TCD29_DOFF,
    #[doc = "0x13b6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd29_citer_elinkno: TCD29_CITER_ELINKNO,
    #[doc = "0x13b8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd29_dlastsga: TCD29_DLASTSGA,
    #[doc = "0x13bc - TCD Control and Status"]
    pub tcd29_csr: TCD29_CSR,
    #[doc = "0x13be - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd29_biter_elinkno: TCD29_BITER_ELINKNO,
    #[doc = "0x13c0 - TCD Source Address"]
    pub tcd30_saddr: TCD30_SADDR,
    #[doc = "0x13c4 - TCD Signed Source Address Offset"]
    pub tcd30_soff: TCD30_SOFF,
    #[doc = "0x13c6 - TCD Transfer Attributes"]
    pub tcd30_attr: TCD30_ATTR,
    #[doc = "0x13c8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd30_nbytes_mlno: TCD30_NBYTES_MLNO,
    #[doc = "0x13cc - TCD Last Source Address Adjustment"]
    pub tcd30_slast: TCD30_SLAST,
    #[doc = "0x13d0 - TCD Destination Address"]
    pub tcd30_daddr: TCD30_DADDR,
    #[doc = "0x13d4 - TCD Signed Destination Address Offset"]
    pub tcd30_doff: TCD30_DOFF,
    #[doc = "0x13d6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd30_citer_elinkno: TCD30_CITER_ELINKNO,
    #[doc = "0x13d8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd30_dlastsga: TCD30_DLASTSGA,
    #[doc = "0x13dc - TCD Control and Status"]
    pub tcd30_csr: TCD30_CSR,
    #[doc = "0x13de - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd30_biter_elinkno: TCD30_BITER_ELINKNO,
    #[doc = "0x13e0 - TCD Source Address"]
    pub tcd31_saddr: TCD31_SADDR,
    #[doc = "0x13e4 - TCD Signed Source Address Offset"]
    pub tcd31_soff: TCD31_SOFF,
    #[doc = "0x13e6 - TCD Transfer Attributes"]
    pub tcd31_attr: TCD31_ATTR,
    #[doc = "0x13e8 - TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
    pub tcd31_nbytes_mlno: TCD31_NBYTES_MLNO,
    #[doc = "0x13ec - TCD Last Source Address Adjustment"]
    pub tcd31_slast: TCD31_SLAST,
    #[doc = "0x13f0 - TCD Destination Address"]
    pub tcd31_daddr: TCD31_DADDR,
    #[doc = "0x13f4 - TCD Signed Destination Address Offset"]
    pub tcd31_doff: TCD31_DOFF,
    #[doc = "0x13f6 - TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd31_citer_elinkno: TCD31_CITER_ELINKNO,
    #[doc = "0x13f8 - TCD Last Destination Address Adjustment/Scatter Gather Address"]
    pub tcd31_dlastsga: TCD31_DLASTSGA,
    #[doc = "0x13fc - TCD Control and Status"]
    pub tcd31_csr: TCD31_CSR,
    #[doc = "0x13fe - TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
    pub tcd31_biter_elinkno: TCD31_BITER_ELINKNO,
}
#[doc = "Control Register"]
pub struct CR {
    register: VolatileCell<u32>,
}
#[doc = "Control Register"]
pub mod cr;
#[doc = "Error Status Register"]
pub struct ES {
    register: VolatileCell<u32>,
}
#[doc = "Error Status Register"]
pub mod es;
#[doc = "Enable Request Register"]
pub struct ERQ {
    register: VolatileCell<u32>,
}
#[doc = "Enable Request Register"]
pub mod erq;
#[doc = "Enable Error Interrupt Register"]
pub struct EEI {
    register: VolatileCell<u32>,
}
#[doc = "Enable Error Interrupt Register"]
pub mod eei;
#[doc = "Clear Enable Error Interrupt Register"]
pub struct CEEI {
    register: VolatileCell<u8>,
}
#[doc = "Clear Enable Error Interrupt Register"]
pub mod ceei;
#[doc = "Set Enable Error Interrupt Register"]
pub struct SEEI {
    register: VolatileCell<u8>,
}
#[doc = "Set Enable Error Interrupt Register"]
pub mod seei;
#[doc = "Clear Enable Request Register"]
pub struct CERQ {
    register: VolatileCell<u8>,
}
#[doc = "Clear Enable Request Register"]
pub mod cerq;
#[doc = "Set Enable Request Register"]
pub struct SERQ {
    register: VolatileCell<u8>,
}
#[doc = "Set Enable Request Register"]
pub mod serq;
#[doc = "Clear DONE Status Bit Register"]
pub struct CDNE {
    register: VolatileCell<u8>,
}
#[doc = "Clear DONE Status Bit Register"]
pub mod cdne;
#[doc = "Set START Bit Register"]
pub struct SSRT {
    register: VolatileCell<u8>,
}
#[doc = "Set START Bit Register"]
pub mod ssrt;
#[doc = "Clear Error Register"]
pub struct CERR {
    register: VolatileCell<u8>,
}
#[doc = "Clear Error Register"]
pub mod cerr;
#[doc = "Clear Interrupt Request Register"]
pub struct CINT {
    register: VolatileCell<u8>,
}
#[doc = "Clear Interrupt Request Register"]
pub mod cint;
#[doc = "Interrupt Request Register"]
pub struct INT {
    register: VolatileCell<u32>,
}
#[doc = "Interrupt Request Register"]
pub mod int;
#[doc = "Error Register"]
pub struct ERR {
    register: VolatileCell<u32>,
}
#[doc = "Error Register"]
pub mod err;
#[doc = "Hardware Request Status Register"]
pub struct HRS {
    register: VolatileCell<u32>,
}
#[doc = "Hardware Request Status Register"]
pub mod hrs;
#[doc = "Enable Asynchronous Request in Stop Register"]
pub struct EARS {
    register: VolatileCell<u32>,
}
#[doc = "Enable Asynchronous Request in Stop Register"]
pub mod ears;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI3 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri3;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI2 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri2;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI1 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri1;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI0 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri0;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI7 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri7;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI6 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri6;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI5 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri5;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI4 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri4;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI11 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri11;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI10 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri10;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI9 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri9;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI8 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri8;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI15 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri15;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI14 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri14;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI13 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri13;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI12 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri12;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI19 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri19;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI18 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri18;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI17 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri17;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI16 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri16;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI23 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri23;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI22 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri22;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI21 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri21;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI20 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri20;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI27 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri27;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI26 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri26;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI25 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri25;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI24 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri24;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI31 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri31;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI30 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri30;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI29 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri29;
#[doc = "Channel n Priority Register"]
pub struct DCHPRI28 {
    register: VolatileCell<u8>,
}
#[doc = "Channel n Priority Register"]
pub mod dchpri28;
#[doc = "TCD Source Address"]
pub struct TCD0_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd0_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD0_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd0_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD0_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd0_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD0_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd0_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD0_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd0_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD0_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd0_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD0_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd0_slast;
#[doc = "TCD Destination Address"]
pub struct TCD0_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd0_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD0_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd0_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD0_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd0_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD0_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd0_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD0_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd0_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD0_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd0_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD0_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd0_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD0_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd0_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD1_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd1_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD1_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd1_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD1_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd1_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD1_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd1_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD1_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd1_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD1_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd1_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD1_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd1_slast;
#[doc = "TCD Destination Address"]
pub struct TCD1_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd1_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD1_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd1_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD1_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd1_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD1_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd1_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD1_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd1_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD1_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd1_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD1_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd1_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD1_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd1_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD2_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd2_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD2_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd2_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD2_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd2_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD2_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd2_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD2_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd2_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD2_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd2_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD2_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd2_slast;
#[doc = "TCD Destination Address"]
pub struct TCD2_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd2_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD2_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd2_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD2_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd2_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD2_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd2_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD2_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd2_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD2_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd2_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD2_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd2_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD2_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd2_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD3_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd3_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD3_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd3_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD3_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd3_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD3_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd3_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD3_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd3_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD3_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd3_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD3_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd3_slast;
#[doc = "TCD Destination Address"]
pub struct TCD3_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd3_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD3_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd3_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD3_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd3_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD3_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd3_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD3_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd3_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD3_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd3_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD3_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd3_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD3_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd3_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD4_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd4_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD4_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd4_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD4_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd4_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD4_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd4_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD4_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd4_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD4_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd4_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD4_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd4_slast;
#[doc = "TCD Destination Address"]
pub struct TCD4_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd4_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD4_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd4_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD4_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd4_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD4_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd4_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD4_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd4_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD4_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd4_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD4_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd4_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD4_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd4_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD5_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd5_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD5_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd5_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD5_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd5_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD5_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd5_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD5_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd5_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD5_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd5_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD5_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd5_slast;
#[doc = "TCD Destination Address"]
pub struct TCD5_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd5_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD5_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd5_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD5_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd5_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD5_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd5_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD5_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd5_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD5_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd5_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD5_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd5_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD5_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd5_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD6_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd6_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD6_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd6_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD6_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd6_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD6_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd6_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD6_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd6_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD6_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd6_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD6_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd6_slast;
#[doc = "TCD Destination Address"]
pub struct TCD6_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd6_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD6_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd6_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD6_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd6_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD6_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd6_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD6_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd6_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD6_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd6_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD6_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd6_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD6_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd6_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD7_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd7_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD7_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd7_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD7_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd7_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD7_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd7_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD7_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd7_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD7_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd7_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD7_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd7_slast;
#[doc = "TCD Destination Address"]
pub struct TCD7_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd7_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD7_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd7_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD7_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd7_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD7_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd7_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD7_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd7_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD7_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd7_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD7_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd7_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD7_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd7_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD8_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd8_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD8_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd8_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD8_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd8_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD8_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd8_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD8_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd8_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD8_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd8_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD8_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd8_slast;
#[doc = "TCD Destination Address"]
pub struct TCD8_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd8_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD8_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd8_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD8_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd8_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD8_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd8_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD8_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd8_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD8_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd8_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD8_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd8_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD8_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd8_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD9_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd9_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD9_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd9_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD9_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd9_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD9_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd9_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD9_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd9_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD9_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd9_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD9_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd9_slast;
#[doc = "TCD Destination Address"]
pub struct TCD9_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd9_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD9_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd9_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD9_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd9_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD9_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd9_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD9_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd9_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD9_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd9_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD9_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd9_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD9_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd9_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD10_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd10_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD10_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd10_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD10_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd10_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD10_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd10_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD10_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd10_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD10_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd10_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD10_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd10_slast;
#[doc = "TCD Destination Address"]
pub struct TCD10_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd10_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD10_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd10_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD10_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd10_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD10_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd10_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD10_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd10_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD10_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd10_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD10_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd10_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD10_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd10_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD11_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd11_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD11_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd11_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD11_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd11_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD11_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd11_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD11_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd11_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD11_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd11_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD11_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd11_slast;
#[doc = "TCD Destination Address"]
pub struct TCD11_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd11_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD11_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd11_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD11_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd11_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD11_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd11_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD11_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd11_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD11_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd11_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD11_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd11_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD11_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd11_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD12_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd12_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD12_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd12_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD12_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd12_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD12_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd12_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD12_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd12_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD12_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd12_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD12_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd12_slast;
#[doc = "TCD Destination Address"]
pub struct TCD12_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd12_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD12_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd12_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD12_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd12_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD12_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd12_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD12_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd12_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD12_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd12_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD12_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd12_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD12_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd12_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD13_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd13_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD13_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd13_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD13_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd13_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD13_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd13_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD13_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd13_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD13_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd13_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD13_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd13_slast;
#[doc = "TCD Destination Address"]
pub struct TCD13_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd13_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD13_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd13_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD13_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd13_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD13_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd13_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD13_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd13_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD13_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd13_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD13_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd13_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD13_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd13_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD14_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd14_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD14_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd14_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD14_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd14_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD14_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd14_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD14_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd14_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD14_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd14_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD14_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd14_slast;
#[doc = "TCD Destination Address"]
pub struct TCD14_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd14_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD14_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd14_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD14_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd14_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD14_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd14_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD14_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd14_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD14_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd14_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD14_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd14_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD14_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd14_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD15_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd15_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD15_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd15_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD15_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd15_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD15_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd15_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD15_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd15_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD15_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd15_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD15_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd15_slast;
#[doc = "TCD Destination Address"]
pub struct TCD15_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd15_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD15_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd15_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD15_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd15_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD15_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd15_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD15_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd15_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD15_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd15_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD15_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd15_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD15_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd15_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD16_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd16_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD16_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd16_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD16_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd16_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD16_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd16_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD16_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd16_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD16_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd16_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD16_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd16_slast;
#[doc = "TCD Destination Address"]
pub struct TCD16_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd16_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD16_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd16_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD16_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd16_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD16_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd16_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD16_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd16_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD16_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd16_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD16_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd16_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD16_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd16_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD17_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd17_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD17_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd17_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD17_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd17_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD17_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd17_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD17_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd17_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD17_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd17_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD17_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd17_slast;
#[doc = "TCD Destination Address"]
pub struct TCD17_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd17_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD17_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd17_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD17_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd17_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD17_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd17_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD17_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd17_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD17_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd17_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD17_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd17_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD17_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd17_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD18_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd18_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD18_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd18_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD18_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd18_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD18_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd18_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD18_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd18_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD18_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd18_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD18_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd18_slast;
#[doc = "TCD Destination Address"]
pub struct TCD18_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd18_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD18_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd18_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD18_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd18_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD18_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd18_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD18_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd18_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD18_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd18_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD18_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd18_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD18_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd18_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD19_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd19_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD19_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd19_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD19_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd19_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD19_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd19_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD19_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd19_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD19_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd19_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD19_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd19_slast;
#[doc = "TCD Destination Address"]
pub struct TCD19_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd19_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD19_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd19_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD19_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd19_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD19_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd19_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD19_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd19_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD19_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd19_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD19_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd19_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD19_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd19_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD20_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd20_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD20_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd20_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD20_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd20_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD20_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd20_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD20_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd20_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD20_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd20_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD20_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd20_slast;
#[doc = "TCD Destination Address"]
pub struct TCD20_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd20_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD20_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd20_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD20_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd20_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD20_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd20_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD20_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd20_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD20_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd20_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD20_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd20_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD20_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd20_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD21_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd21_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD21_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd21_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD21_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd21_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD21_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd21_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD21_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd21_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD21_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd21_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD21_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd21_slast;
#[doc = "TCD Destination Address"]
pub struct TCD21_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd21_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD21_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd21_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD21_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd21_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD21_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd21_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD21_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd21_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD21_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd21_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD21_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd21_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD21_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd21_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD22_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd22_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD22_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd22_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD22_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd22_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD22_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd22_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD22_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd22_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD22_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd22_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD22_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd22_slast;
#[doc = "TCD Destination Address"]
pub struct TCD22_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd22_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD22_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd22_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD22_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd22_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD22_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd22_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD22_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd22_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD22_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd22_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD22_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd22_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD22_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd22_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD23_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd23_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD23_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd23_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD23_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd23_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD23_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd23_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD23_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd23_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD23_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd23_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD23_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd23_slast;
#[doc = "TCD Destination Address"]
pub struct TCD23_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd23_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD23_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd23_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD23_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd23_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD23_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd23_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD23_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd23_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD23_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd23_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD23_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd23_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD23_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd23_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD24_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd24_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD24_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd24_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD24_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd24_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD24_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd24_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD24_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd24_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD24_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd24_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD24_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd24_slast;
#[doc = "TCD Destination Address"]
pub struct TCD24_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd24_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD24_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd24_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD24_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd24_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD24_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd24_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD24_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd24_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD24_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd24_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD24_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd24_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD24_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd24_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD25_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd25_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD25_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd25_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD25_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd25_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD25_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd25_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD25_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd25_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD25_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd25_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD25_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd25_slast;
#[doc = "TCD Destination Address"]
pub struct TCD25_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd25_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD25_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd25_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD25_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd25_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD25_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd25_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD25_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd25_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD25_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd25_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD25_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd25_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD25_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd25_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD26_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd26_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD26_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd26_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD26_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd26_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD26_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd26_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD26_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd26_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD26_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd26_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD26_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd26_slast;
#[doc = "TCD Destination Address"]
pub struct TCD26_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd26_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD26_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd26_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD26_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd26_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD26_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd26_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD26_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd26_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD26_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd26_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD26_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd26_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD26_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd26_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD27_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd27_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD27_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd27_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD27_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd27_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD27_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd27_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD27_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd27_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD27_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd27_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD27_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd27_slast;
#[doc = "TCD Destination Address"]
pub struct TCD27_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd27_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD27_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd27_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD27_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd27_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD27_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd27_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD27_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd27_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD27_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd27_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD27_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd27_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD27_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd27_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD28_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd28_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD28_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd28_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD28_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd28_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD28_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd28_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD28_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd28_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD28_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd28_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD28_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd28_slast;
#[doc = "TCD Destination Address"]
pub struct TCD28_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd28_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD28_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd28_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD28_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd28_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD28_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd28_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD28_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd28_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD28_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd28_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD28_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd28_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD28_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd28_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD29_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd29_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD29_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd29_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD29_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd29_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD29_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd29_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD29_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd29_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD29_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd29_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD29_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd29_slast;
#[doc = "TCD Destination Address"]
pub struct TCD29_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd29_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD29_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd29_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD29_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd29_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD29_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd29_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD29_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd29_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD29_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd29_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD29_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd29_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD29_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd29_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD30_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd30_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD30_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd30_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD30_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd30_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD30_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd30_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD30_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd30_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD30_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd30_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD30_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd30_slast;
#[doc = "TCD Destination Address"]
pub struct TCD30_DADDR {
    register: VolatileCellz<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd30_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD30_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd30_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD30_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd30_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD30_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd30_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD30_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd30_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD30_CSR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Control and Status"]
pub mod tcd30_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD30_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd30_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD30_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd30_biter_elinkyes;
#[doc = "TCD Source Address"]
pub struct TCD31_SADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Source Address"]
pub mod tcd31_saddr;
#[doc = "TCD Signed Source Address Offset"]
pub struct TCD31_SOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Source Address Offset"]
pub mod tcd31_soff;
#[doc = "TCD Transfer Attributes"]
pub struct TCD31_ATTR {
    register: VolatileCell<u16>,
}
#[doc = "TCD Transfer Attributes"]
pub mod tcd31_attr;
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub struct TCD31_NBYTES_MLNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Minor Byte Count (Minor Loop Mapping Disabled)"]
pub mod tcd31_nbytes_mlno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub struct TCD31_NBYTES_MLOFFNO {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping Enabled and Offset Disabled)"]
pub mod tcd31_nbytes_mloffno;
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub struct TCD31_NBYTES_MLOFFYES {
    register: VolatileCell<u32>,
}
#[doc = "TCD Signed Minor Loop Offset (Minor Loop Mapping and Offset Enabled)"]
pub mod tcd31_nbytes_mloffyes;
#[doc = "TCD Last Source Address Adjustment"]
pub struct TCD31_SLAST {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Source Address Adjustment"]
pub mod tcd31_slast;
#[doc = "TCD Destination Address"]
pub struct TCD31_DADDR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Destination Address"]
pub mod tcd31_daddr;
#[doc = "TCD Signed Destination Address Offset"]
pub struct TCD31_DOFF {
    register: VolatileCell<u16>,
}
#[doc = "TCD Signed Destination Address Offset"]
pub mod tcd31_doff;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD31_CITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd31_citer_elinkno;
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD31_CITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Current Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd31_citer_elinkyes;
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub struct TCD31_DLASTSGA {
    register: VolatileCell<u32>,
}
#[doc = "TCD Last Destination Address Adjustment/Scatter Gather Address"]
pub mod tcd31_dlastsga;
#[doc = "TCD Control and Status"]
pub struct TCD31_CSR {
    register: VolatileCell<u32>,
}
#[doc = "TCD Control and Status"]
pub mod tcd31_csr;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub struct TCD31_BITER_ELINKNO {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Disabled)"]
pub mod tcd31_biter_elinkno;
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub struct TCD31_BITER_ELINKYES {
    register: VolatileCell<u16>,
}
#[doc = "TCD Beginning Minor Loop Link, Major Loop Count (Channel Linking Enabled)"]
pub mod tcd31_biter_elinkyes;
